*Features:*

\*\* Ideal for all general purpose drilling, honing, reaming, and hole sawing

\*\* Impact resistant & cold insulated composite housing produce a great feeling and

durable tool with lightweight & quieter operation

\*\* Excellent power-to-weight ratio gets the job done with less fatigue

 \*\* Dust free reverse lever positioned for one-hand operation

 \*\* Variable speed throttle for starting hole easily

\*\* With 3/8” Jacobs drill chuck

***Specification :***

* Chuck Capacity: 3/8” (10mm)
* Free Speed: 1,800 RPM
* Horse Power: 0.35 HP
* Spindle Thread: 3/8”-24T
* Air Inlet: 1/4” NPT (PT)
* Recommend air pressure: 90 PSI
* Min. Air Hose: 3/8” (10mm) I.D.
* Net Weight: 0.97 KGS (2.1 LBS)
* Overall Length: 165 MM (6.49”)